|  |
| --- |
| Photo displaying partial image of two pie charts on a canvas-textured page |
| PO3\_DGW  Customer System Requirements Specifications Document |
| |  |  |  | | --- | --- | --- | | Bassem Ezzat | 1/24/20 | Mohammed ElSayed | |

Contents

[Table of history 2](#_Toc31272928)

[1. Introduction 3](#_Toc31272929)

[1.1. Purpose 3](#_Toc31272930)

[1.2. Document Abbreviation 3](#_Toc31272931)

[1.3. Intended audience and reading suggestions 3](#_Toc31272932)

[1.4. Project Scope 3](#_Toc31272933)

[1.5. References 3](#_Toc31272934)

[2. Overall Description 4](#_Toc31272935)

[2.1. Product features 4](#_Toc31272936)

[2.2. Operation environment 4](#_Toc31272937)

[2.3. Design and Implementation constraints 4](#_Toc31272938)

[3. System Features 5](#_Toc31272939)

[3.1. Functional requirements 5](#_Toc31272940)

[3.1.1. FUNC\_PO3\_DGW\_CYRS\_01\_V01 5](#_Toc31272941)

[3.1.2. FUNC\_PO3\_DGW\_CYRS\_02\_V01 5](#_Toc31272942)

[3.1.3. FUNC\_PO3\_DGW\_CYRS\_03\_V01 5](#_Toc31272943)

[3.1.4. FUNC\_PO3\_DGW\_CYRS\_04\_V01 5](#_Toc31272944)

[3.1.5. FUNC\_PO3\_DGW\_CYRS\_05\_V01 6](#_Toc31272945)

[3.1.6. FUNC\_PO3\_DGW\_CYRS\_06\_V01 6](#_Toc31272946)

[3.1.7. FUNC\_PO3\_DGW\_CYRS\_07\_V02 6](#_Toc31272947)

[3.1.8. FUNC\_PO3\_DGW\_CYRS\_08\_V01 6](#_Toc31272948)

[3.1.9. FUNC\_PO3\_DGW\_CYRS\_09\_V01 6](#_Toc31272949)

[3.2. Hardware Requirements 8](#_Toc31272950)

[3.2.1. HW\_PO3\_DGW\_CYRS\_01\_V01 8](#_Toc31272951)

[3.2.2. HW\_PO3\_DGW\_CYRS\_02\_V01 8](#_Toc31272952)

[3.2.3. HW\_PO3\_DGW\_CYRS\_03\_V01 8](#_Toc31272953)

# **Table of history**

|  |  |  |  |
| --- | --- | --- | --- |
| *Version* | *Author(s)* | *Date* | *Changes* |
| 0.0 | - Bassem Ezzat  - Mohammed Elsayed | January 24, 2020 | Creation of CYRS document |
| 0.1 | - Bassem Ezzat  - Mohammed Elsayed  - Mariam El-Shakafi | January 25, 2020 | Added further details to requirements based on SIQ answers |
| 0.2 | - Mariam El-Shakafi | January 30, 2020 | Updated FUNC\_ PO3\_DGW\_CYRS\_07 |

# **Introduction**

* 1. Purpose

This document aims to clarify the CRS document and list a customer requirement specification to design a digital watch.

* 1. Document Abbreviation

|  |  |
| --- | --- |
| CYRS | Customer System Requirement Specifications |
| CRS | Customer Requirement Specifications |
| ERD | Entery relational digram |
| SIQ | Software interactive questionnaire |
| FUNC | Functional button |
| INC | Increment button |
| DEC | Decrement |

* 1. Intended audience and reading suggestions

This project is a prototype for a digital watch, and it is applicable to be a commercial product. This has been implemented under the guidance of ITI’s trainers.

* 1. Project Scope

The purpose of this project is to create modern stunning digital watch.

* 1. References

Not available yet

1. Overall Description
   1. Product features

The major feature of the digital watch as listed below.

* Display time with 12 AM/PM format.
* Alarm to set according to user input.
* Stopwatch (Start, Stop).
* Three buttons to control the system:
  + MODE
  + FUNC1
  + FUNC2
  1. Operation environment

Operating environments for the digital watch are houses, offices, shops, and hotels.

* 1. Design and Implementation constraints
* Software layer design
* Hardware components selection

1. System Features
   1. Functional requirements
      1. FUNC\_PO3\_DGW\_CYRS\_01\_V01

Display Time Mode:

* The software shall enter Display Time mode when current mode is Stopwatch mode and MODE button is pressed, or when system is powered-up.
* The software shall display the time in HH:MM:SS AM/PM format.
  + 1. FUNC\_PO3\_DGW\_CYRS\_02\_V01

Adjust Time:

* To adjust the time (Minutes), press FUNC1 button once, so the minutes start blinking to indicate that it can be modified using FUNC2 button.
* To adjust the time (Hours), press FUNC1 button twice, so the hours start blinking to indicate that it can be modified using FUNC2 button.
* To adjust the time (AM/PM), press FUNC1 button a third time, so the format starts blinking to indicate that it can be modified using FUNC2 button.
* To apply adjustments, press FUNC1 button for a fourth time.
  + 1. FUNC\_PO3\_DGW\_CYRS\_03\_V01

Alarm Mode:

* The software shall enter Alarm mode when current mode is Display Time mode and MODE button is pressed.
* The software shall display the time in HH:MM:SS AM/PM format until Alarm time is reached.
  + 1. FUNC\_PO3\_DGW\_CYRS\_04\_V01

Set Alarm:

* To adjust alarm time (Minutes), press FUNC1 button once, so the minutes start blinking to indicate that it can be modified using FUNC2 button.
* To adjust alarm time (Hours), press FUNC1 button twice, so the hours start blinking to indicate that it can be modified using FUNC2 button.
* To adjust alarm time (AM/PM), press FUNC1 button a third time, so the format starts blinking to indicate that it can be modified using FUNC2 button.
* To set alarm, press FUNC1 button for a fourth time.
  + 1. FUNC\_PO3\_DGW\_CYRS\_05\_V01

Buzzer:

* The software shall trigger a buzzer with notification when alarm time is reached in Alarm mode.
* The software shall stop buzzer when FUNC2 button is pressed.
  + 1. FUNC\_PO3\_DGW\_CYRS\_06\_V01

Stopwatch Mode:

* The software shall enter Stopwatch mode when current mode is Alarm mode and MODE button is pressed.
* The software shall display 00:00:00.
  + 1. FUNC\_PO3\_DGW\_CYRS\_07\_V02

Start Counting:

The software shall start counting when FUNC1 button is pressed in Stopwatch mode initial state, or paused state.

* + 1. FUNC\_PO3\_DGW\_CYRS\_08\_V01

Stop Counting:

The software shall stop counting when FUNC1 button is pressed in Stopwatch mode running state.

* + 1. FUNC\_PO3\_DGW\_CYRS\_09\_V01

Reset Counting:

The software shall reset counter to 00:00:00 when FUNC2 button is pressed in Stopwatch mode.

|  |  |
| --- | --- |
| **CYRS REQUIREMENT** | **CRS REQUIREMENT** |
| FUNC\_ PO3\_DGW\_CYRS\_01\_V01 | Display the time with 12 AM/PM format |
| FUNC\_ PO3\_DGW\_CYRS\_02\_V01 | User can adjust time using buttons |
| FUNC\_ PO3\_DGW\_CYRS\_04\_V01 | Alarm to be set as per the input |
| FUNC\_ PO3\_DGW\_CYRS\_05\_V01 | When alarm time is reached, a buzzer with notification is triggered |
| FUNC\_ PO3\_DGW\_CYRS\_07\_V01  FUNC\_ PO3\_DGW\_CYRS\_08\_V01  FUNC\_ PO3\_DGW\_CYRS\_09\_V01 | Stopwatch with “start, stop, and Reset” |
| FUNC\_ PO3\_DGW\_CYRS\_06\_V01 | Reset all digits once entering stopwatch mode |
| FUNC\_ PO3\_DGW\_CYRS\_01\_V01  FUNC\_ PO3\_DGW\_CYRS\_03\_V01  FUNC\_ PO3\_DGW\_CYRS\_06\_V01 | User can control digital watch modes using one button |

* 1. Hardware Requirements
     1. HW\_PO3\_DGW\_CYRS\_01\_V01

Display:

Time shall be displayed using LCD.

* + 1. HW\_PO3\_DGW\_CYRS\_02\_V01

Control:

The user shall control the digital watch using ONLY 3 buttons.

* + 1. HW\_PO3\_DGW\_CYRS\_03\_V01

Power source:

The system shall be powered using batteries.